
**ELECTRIC CURTAIN INSTRUCTIONS**

1. AFTER INSTALLATION AND RECEPTION, PLEASE FIRST MOVE THE DROOP ROD FIXING CLIP TO BOTH SIDES AND REMOVE THE REAR SCREEN BEFORE USE.
2. CHECK TO ENSURE THAT THERE IS NO PROBLEM WITH THE POWER SUPPLY AND CONNECT THE POWER SUPPLY.
3. PRESS THE MANUAL SWITCH TO LIFT THE SCREEN, AND PUT THE SWITCH IN THE CENTER STOP POSITION WHEN NOT IN USE.
4. THE LIMIT POINT OF THE SCREEN HAS BEEN DEBUGGED BEFORE LEAVING THE FACTORY.NO SPECIAL NEEDS, PLEASE DO NOT DISASSEMBLE AND MOBILIZE WITHOUT AUTHORIZATION IF THE LIMIT SHIFT CAUSED BY LARGE VIBRATION DURING TRANSPORTATION NEEDS TO BE MOBILIZED,

IT IS NECESSARY TO STRICTLY FOLLOW THE FOLLOWING METHODS AND STEPS,

OTHERWISE IT WILL CAUSE DAMAGE.

(1) ENTER SETUP MODE

UNDER NORMAL CONDITIONS (RED LIGHT), PRESS AND HOLD THE UP BUTTON  
 (THE ONE CLOSEST TO THE LIGHT) UNTIL THE BLUE LIGHT COMES ON AND LET GO.

(2) SET THE LOWER BORDER

THIS TIME THROUGH THE UP AND DOWN KEYS TO SET THE LOWER BOUNDARY.

(3) STORAGE LOWER BOUNDARY

AFTER THE LOWER BOUNDARY IS DETERMINED, LONG PRESS THE UPPER BUTTON FOR 3 SECONDS, THE BLUE LIGHT FLASHES AND RAISES YOUR HAND, INDICATING THAT THE LOWER BOUNDARY MEMORY IS SUCCESSFUL.

(4) ESTABLISHMENT OF UPPER BOUNDARY

AT THIS TIME, SHORT PRESS THE UP BUTTON, THE SCREEN UP, WHEN THE SCREEN IS CLOSED, SHORT PRESS UP BUTTON TO STOP

(5) PRESERVATION OF WITHDRAWAL

AFTER SETTING THE LOWER BOUNDARY AND UPPER BOUNDARY, LONG PRESS THE UPPER KEY FOR 3 SECONDS, THE BLUE LIGHT FLASHES, RAISE YOUR HAND, THE BLUE LIGHT TURNS RED,AND ENTER THE NORMAL WORKING STATE.

1. **RECOMMENDED INSTALLATION METHODS**

|  |  |  |  |
| --- | --- | --- | --- |
| 1.WALL MOUNTING    111  LET THE SCREW THROUGH THE WALL HANGING HOLE OF THE END CAP | 1. CEILING MOUNTING   222   PUT THE RING ON THE HOOK IN THE CEILING | 3.WALL BRACKET INSTALLATION | 4.HIDDEN INSTALLATION |
| O | O |
| IT IS RECOMMENDED TO USE A PROFESSIONAL BRACKET | LEAVE ENOUGH SPACE TO HIDE THE PROJECTION SCREEN |